
WELD MESH FENCE PANEL

ROUGH SKETCH ONLY FOR INDICATION OF ASSEMBLY

WILL BE ASSEMBLED IN AUSTRALIA FOR TO MAKE PACKING FOR SHIPPING EASY
























STAY BAR one bar & D Clamp per 6 panels





Plain Galvanised Plain Pipe


48.5mmØ


2mm thickness


2000 mm long





3 FOLDS GALVANISED WELD MESH 5MM DIAMETER 


REFER TO OTHER DETAILS & DRAWING FOR DIMENTIONS





PORTABLE BASES





D CLAMP





Hole 13mm straight trough both sides 6mm from edge








